**B.PRO COOK induction hob**

**with a rectangular cooking zone**

**BC SIH 5000**

**Dimensions:**

Length: 620 mm

Width: 400 mm

Height: 240 mm

**Housing design:**

The surface induction hob is made completely of micro-polished stainless steel (AISI 304), equipped with height-adjustable rotating feet. A 6 mm-thick glass ceramic surface is integrated flush in the cover and grouted with high-temperature resistant, highly elastic sealing compound. The glass ceramic surface has a rectangular marking. Pots and pans can be placed anywhere within this area. The air intake opening is below the unit and is via a removable air filter. The extracted air is removed via ventilation slits on the back of the top surface. The unit is designed to ensure that it can be positioned against a directly adjacent rear wall.

An operating area, moulded toward the rear for improved viewing and operator ergonomics, is seamlessly installed on the front panel to hold the output regulator.

**Electrical equipment:**

The unit is equipped with a microprocessor-controlled E.G.O. induction generator. The cooking surface on the rectangular cooking zone is 220 x 447 mm. 1 heating zone with 2 induction coils, each measuring 220 x 220 mm. Automatic pot detection from a pot/pan diameter of 120 mm. Continuous power control is carried out with an integrated rotary knob installed in the operating area. An indicator light provides information on the operating mode and the error code in the event of faults. The unit is completely electrically wired and equipped with a 1.5 m connection cable with a 400 V, 16 A CEE plug which exits at a downward angle on the underside.

**Accessories/options:**

* Glass-ceramic cleaning scraper

Order No.: 568 489

* Clamping bar for bridging the gap to other B.PRO COOK units

Order No.: 574 298

**Technical data:**

Material: Stainles steel (AISI 304)

Glass-ceramic

Weight: approx. 27 kg

Protection type: IP X4

Heat emission sensitive: 0.35 kW

Heat emission latent: 0.14 kW

Cooking zone: 220 x 447 mm

Generator model: E.G.O.- QUAD Plus Duo Tray

Connected load: 400 V / 3N PE AC

50-60 Hz / 5.0 kW  
(2 x 2.5 kW)

**Special features:**

* High efficiency through induction technology
* Low heat dissipation
* Energy-saving cooking
* Micro-polished surface made of stainless steel
* Angled operating area
* High-performance induction generator  
  made by E.G.O.

**Make:**

Manufacturer: B.PRO

Type: BC SIH 5000

Order No.: 574 200